|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Name | |  | | Job Title | |  | | | |
| Payroll No. |  | | Hospital |  | | | | Ward/Dept. |  |
| PAPR Make | Drager | | | | PAPR Model | | X-Plore 8000 | | |

|  |  |  |
| --- | --- | --- |
| **I am able to undertake the following** | **Aide Memoir Location** | **Competent**  **(Initial)** |
| Attach belt to blower unit | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Charge the battery (insert and remove from charger) | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Insert and remove battery from blower, checking fully charged | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Check gaskets/O rings are in situ (filter & hoses) | [PAPR Self Learning Pack](https://www.nhsggc.org.uk/media/264729/papr-self-learning-pack.pptx) |  |
| Insert/attached filters | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Connect hose to blower unit | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Connect hose to head top | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Operate the PAPR system | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Describe the warning alarms on the Blower (battery and filter) and the action to take if triggered | [PAPR Self Learning Pack](https://www.nhsggc.org.uk/media/264729/papr-self-learning-pack.pptx) |  |
| Don hood/blower unit | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Check and adjust flow rate | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Doff hood and blower unit | <https://www.youtube.com/watch?v=HjfxJ2ewK0I> |  |
| Decontaminate PAPR system | [PAPR HRConnect webpage - IPC](https://www.nhsggc.org.uk/working-with-us/hr-connect/health-safety/policies-guidance-documents-forms/personal-protective-equipment/powered-air-purifying-respirators-papr/) |  |
| Clean the PAPR elements | [PAPR HRConnect webpage - IPC](https://www.nhsggc.org.uk/working-with-us/hr-connect/health-safety/policies-guidance-documents-forms/personal-protective-equipment/powered-air-purifying-respirators-papr/) |  |
| The 6 steps to effective hand hygiene | [Chapter 1.2 of the NIPCM](http://www.nipcm.hps.scot.nhs.uk/chapter-1-standard-infection-control-precautions-sicps/#a1069) |  |
| I have read and understood the steps to take for effective donning and doffing of PPE associated with use of this PAPR | [PAPR HRConnect webpage - IPC](https://www.nhsggc.org.uk/working-with-us/hr-connect/health-safety/policies-guidance-documents-forms/personal-protective-equipment/powered-air-purifying-respirators-papr/) |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Delegate Signature |  | Date |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Assessors Name | |  | Job Title |  |
| Hospital |  | | Ward/Dept. |  |

|  |  |
| --- | --- |
| **I have observed the above named as being competent in the following activities** | **Assessor (Initials)** |
| How to attach belt to blower unit |  |
| How to charge battery (insert and remove from charger) |  |
| How to insert and remove battery from blower, checking fully charged |  |
| How to check gaskets/O rings are in situ (filter & hoses) |  |
| How to insert/attached filters and check the seal, P3 (type of filter) and expiry date |  |
| How to connect hose to blower unit and undertake check of alarms by covering hose |  |
| How to connect hose to head top |  |
| How to operate the PAPR system |  |
| How to don hood, using loops on the hood with the blower unit switched on throughout |  |
| How to check / adjust flow rate |  |
| How to doff hood, using loops on hood. NB the blower unit to be switched off after removal of hood |  |
| Has accurately described the warning alarms on the unit – battery and filter |  |
| Has accurately described the process for safely doffing and decontaminating the PAPR unit |  |
| Has accurately described when PAPR is to be used and not used – only in AGP zones |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Assessor Signature |  | Date |  |